four steps to update firmware

1, power off

2, copy new firmware two files (lite\_cfg.txt mksLite.bin)to the TF card, and insert the TF card to printer.

3, power on

4, wait 60 seconds. The printer will update firmware automatically.

（If update succeed , two files’ suffix of the two files will change to cur, The two files in the TF card become lite\_cfg.cur   mksLite.cur）

四步更新固件

1. 关机断电
2. 把固件两个文件(lite\_cfg.txt mksLite.bin)拷到TF卡，把卡插入卡槽
3. 通电开机
4. 等待60秒， 固件自动更新。

（如果程序更新成功，两个文件的后缀会变成cur，TF卡里的两个文件变成lite\_cfg.cur   mksLite.cur）